These are step-by-step instructions on how to install the upgrade in an XEGS and What each step does for the Atari Video Signal.

Disclaimer: I am not responsible for you screwing up your computer. You do this upgrade at your own risk.


1 - (Disconnect the RF modulator)

· Simply Cut and Remove all three connections that are sticking out of the back of the RF modulator and connected to the motherboard. The RF Modulator will not work after doing this upgrade anyway.

2 - (Luma)

· The Luma Signal is not that bad in the 8-bit To begin with. it just needs to bypass all the crap that Atari put in front of it. At the Top Leg of Q3 is where you should run a 47ohm Resistor from. Run the other end of the resistor to your Luma Out. A 75ohms Resistor will work but the contrast is better at 47ohms and the yield to the Chroma signal will be smoother. Especially if you want to combine them to Make Composite Video.


3 - (Chroma)

· The Chroma Signal is The Real Culprit Behind the Atari's Video Problems. It's just Plain Over-saturated. Simply Bypassing all the extra Garbage and connecting directly to Pin 21 of the GTIA with a 22uf 16v Cap is Perfect. A Good Place to Find a Connection to Pin 21 is the TOP of R87. Connect the Other End of the Cap to your Chroma Out. There is More to this but I will Explain it in the next Section.


4 - (Chroma Ground out)

· To Make the Chroma Work With Newer TV's (Fix The Vertical Banding issue) is as simple as adding one side of a 75ohm Resistor to the IN Leg (Side Connected to Pin 21 of GTIA) of the 22uf Cap on the Chroma line and the other end of the 75ohm resistor to Ground on the Mainboard. This will Get rid of the vertical Banding (On Most TV's) Which is Caused By DC Voltage in the Signal and an Overly Strong Chroma Signal. [NOTE] Just Remember When Combining the Luma and Chroma to Make Composite Video you must NOT have This 75ohm Resistor Connected as the Chroma Signal Will Not be Strong Enough to Mix Well With The Luma and will cause nasty Red and Green Color Shadows as a result. This is why I have Always Used a Switch to Turn the connection of the 75ohm Resistor on or off as I needed. 

That’s it. You should be ready to go. If you have any questions feel free to Email me at kjmann_Atari@yahoo.com. I’m always happy to help.
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